How to know the SRAM read 1 or 0

Shantonu Debnath

IIEST, Shibpur

When bit low read 0

And when bit bar low read 1

Reference:

1. <https://www.youtube.com/watch?v=k5VBJcUcaWU>
2. <https://www.researchgate.net/post/Sram-read-operation-pspice-netlist>
3. <https://www.youtube.com/watch?v=vlHHFIrTTnA&list=PLfP-D1tg0DI2Sn1DVzGdIeGyuIUjhJ9zp&index=8>